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[bookmark: _GoBack]A Guide to Safety Precautions when first responding to a Road Collision involving a Hybrid or Plug in Electrical vehicles.

1. Ask the driver/owner or witness if the vehicles involved in the collision are Electric Hybrid vehicles?
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2.	Ask them to “Turn the ignition OFF”.
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3.	Remove the Key from the vehicle and place it at least 5 meters away from the vehicle in a safe place, Don’t Lose the key!
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4.	If the vehicle has collision damage “THINK about YOUR SAFETY FIRST” do you need to return to the vehicle?
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5.	Do not push the vehicle or rotate the vehicles wheels until the service plug has been removed by trained personnel.
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6.	Stay safe and wait until a Trained Police officer or Trained recovery agent arrives at the scene.
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