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Use Cisco Routers and Switches to design the above topology and do the required configuration. Make sure you take adequate screenshot and copy the running-configurations to submit as a part of your work. Submit the work in Moodle – Prereq link.
1. Assign IP Address to all the networks:
a. Network A: 192.168.1.0/27
b. Network B: 192.168.2.0/24
c. Network C: 10.10.10.0/30

2. Create a Loopback at R2 with Loopback 1 and assign IP Address 209.209.200.200/32
3. Use Static Routing Protocol to establish communication between Networks. (Do not add Loopback network)
4. Make sure any ping packets that are not specified are routed through Loopback 1.

Submit the work in Moodle
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