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Figure 1: RRAS Enabled (Birmingham)
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Figure 2: ICMP Firewall
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Figure 3: IP Forwarding (London) 
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Figure 4: Routing London
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Figure 5: Domain Creation
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Figure 6: Password Policy
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Figure 7: DNS A Records
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Figure 8: PTR Records
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Figure 9: VPN Ping Test
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Figure 10: DHCP Install
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Figure 11: DHCP IP configuration on client2011 machine using ipconfig /all
[image: ]

Figure 12: Network Configuration Verification using the Ip a Command in Debian
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Figure 13: Network Configuration Verification using the Ip a Command in Debian


Figure 1: RRAS Enabled (Birmingham)
This shows RRAS enabled on Server1. It allows the server to act as a router and forward traffic between networks.
 Figure 2: ICMP Firewall
ICMP was enabled in the firewall to allow ping communication, which is used to test network connectivity.
Figure 3: IP Forwarding (London)
This confirms IP forwarding is enabled, allowing the server to route traffic between different networks.
Figure 4: Routing London
This shows routing configuration on the London server, enabling communication with the Birmingham network.
 Figure 5: Domain Creation
This shows the creation of the mika.acca domain, allowing centralised management and authentication.
 Figure 6: Password Policy
This shows the password policy enforcing security rules like complexity and minimum length.


Figure 7: DNS A Records
A records were created to map hostnames to IP addresses, allowing devices to communicate using names instead of IPs.
Figure 8: PTR Records
PTR records allow reverse DNS lookup, converting IP addresses back to hostnames.
Figure 9: VPN Ping Test
This shows successful ping between networks through VPN, confirming secure connectivity.
 Figure 10: DHCP Install
This shows DHCP installed and authorised to automatically assign IP addresses to clients.
 Figure 11: DHCP IP configuration on client machine using ipconfig /all
The client received an IP address automatically, confirming DHCP is working correctly.
Figure 12: Network Configuration Verification using the Ip a Command in Debian
The image shows the manual configuration of an IP address on a Debian virtual machine, where the IP and subnet mask were defined to enable network communication.
Figure 13: Network Configuration Verification using the Ip a Command in Debian 
The image shows the use of the Ip a command to verify the IP address and the status of network interfaces on the Debian machine.
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