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Lab: IPv4, Subnetting, VLSM and IPv6 Addressing


Understanding IPv4 and IPv6 addressing (word count 1000) 
This part of lab worksheet require you research and write a report on “Features of IPv6”. You may discuss but not limited to structure, address types, advanced functionalities and security.  
Subnetting and VLSM

NOTE: To complete this part you would need full understanding of Lab 10 to 14. 
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Using the Network address 172.16.2.0/24, VLSM the network to support the following requirements: 
Subnet A: 16 hosts       
Subnet B: 2000 hosts  
Subnet C: 6 hosts
Subnet D: 500 hosts
Subnet E: 60 hosts
Subnet F: 180 hosts and Serial links between routers
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Table 1
	Subnet
	Network Address
	Subnet mask
	First Address
	Last Address
	Broadcast Address

	B
	172.16.2.0/21
	255.255.248.0
	172.16.2.1
	172.16.9.254
	172.16.9.255

	D
	172.16.10.0/23
	255.255.254.0
	172.16.10.1
	172.16.11.254
	172.16.11.255

	F
	172.16.12.0/24
	255.255.255.0
	172.16.12.1
	172.16.12.254
	172.16.4.255

	E
	172.16.13.0/25
	255.255.255.128
	172.16.13.1
	172.16.13.62
	172.16.5.63

	A
	172.16.13.64/27
	255.255.255.224
	172.16.13.65
	172.16.13.94
	172.16.13.95

	C
	172.16.13.95/29
	255.255.255.248
	172.16.13.96
	172.16.13.102
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