	Activity to be Assessed
	Assessment Number

	Using power tools 
	3

	Persons undertaking or affected by the activity
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	Employees
	
	Contractor
	
	Public
	
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Power supply – electrocution 
	3
	5
	15

	2
	Dust released – Inhalation, irritates eyes
	4
	3
	12

	3
	Vibration from tool – Hand/arm vibration syndrome 
	5
	3
	15

	4
	Hair or clothing becoming entangled in moving parts
	3
	4
	12

	5
	The tool jamming-hand or arm injury
	3
	3
	9

	6
	
	
	
	

	Existing Control Measures / Additional Control Measures Required

	1
	Use ground fault circuit interrupters

Never use power near any water or live electrical cables

Don’t use extension cables longer than 100ft 
Where practicable only 110v electrical tools will be used.

All power feeds should comply with European or British Standards maintained in  a good condition. 

	2
	Mask and eye protection to be worn when there is a dust hazard. 

	3
	Take regular breaks of at least 10 minutes away from using the tool. 
Hold tools are loosely as possible and in varying positions 

Ensure the tool in use is the correct tool for the job. 

Keep your hands warm while working. 

Select power tools with the lowest vibration level. Use tools with anti-vibration handles. 

	4
	Lose clothing and long hair to be kept clear of moving parts of power tools. 

	5
	Ensure tools are used in accordance with the manufacture’s instructions. 

	6
	

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Electrocution from tool
	2
	5
	10

	2
	Dust causing irritation/inhalation 
	2
	3
	6

	3
	Hand/arm vibration syndrome
	2
	3
	6

	4
	Hair or clothing becoming tangled in moving parts
	2
	4
	8

	5
	Jamming hand or arm injury
	2
	3
	6

	6
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	Reviews
	Key
	

	Review Date: 1.6.20
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 1.6.20
	1   very     unlikely

2   unlikely

3   likely

4   very likely

5   certainty
	1   nuisance

2   minor

3   medical treatment

4   major

5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :1.6.20
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:1.6.20
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	4
	6Y
	8
	10Y

	Review Date :1.6.20
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:1.6.20
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :1.6.20
	
	
	
	Likelihood of Injury

	Reviewed by:1.6.20
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk


