Based on NRM1 - Prepare a cost estimate for the proposed scheme:
The sketch shows a floor plan for a 5-storey office block (for owner occupation) that is proposed to be built in Swansea SA1. A brief Spec. has been issued along with the sketch.
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Substructure
Bored piles reinforced concrete ground beams and precast concrete suspended slab.

Frame and upper floors
In-situ concrete frame with pre-cast concrete suspended slab/ precast concrete stairs.
Façade
280mm cavity walls rendered externally, with coated, double-glazed aluminium windows and doors.
Internally
Hardwood veneered doors, fire resistant to all public and access areas. Plaster and emulsion paint, softwood skirtings, medium quality carpet. Tiling to toilets, bathrooms and WC’s. Suspended ceilings throughout.
Fittings
White bathroom fittings/mirrors.
Heating
Electric central heating and Air Conditioning
Lifts
2 car passenger lift
Externally
Car park is located adjacent to development and will be lightly landscaped. (100 cars max)

Notes:
1. The proposed start date is October 2024. 
2. Data region is Solihull 
3. Data based in Q4 2022 
4. Use Spons 2023 (Moodle)
5. Allow for Tender inflation 
6. Allow for construction inflation
7. Allow for location adjustment
8. No Facilitating works to be included.
9. Use GIFA and Functional Unit method
10. Allow £3500/m2 for toilets 
11. Main Contractors prelims = 10%
12. MC O/H = 11%
13. MC profit = 3%
14. Allow 15% for design team fees (architect, engineer and QS)
15. Allow 2% for planning and approvals
16. All risks allowance = 5%
17. Use NRM1 order of cost estimate format (page 22)
