[bookmark: _GoBack]Technical Drawing Tutorial
Opening a Drawing from a Template
1. Open SolidWorks 2018
2. In the Dialogue box, select Drawing under the New section
3. The Sheet Format/Size Dialogue box should open, select A3 (BSI) and click OK.
4. The Model View Property Manager should appear on the Left hand side of the screen, click the red x
Editing the Sheet Format
1. Right-click anywhere in the drawing sheet, and select Edit Sheet Format. 
2. Zoom in over the title block using the Zoom to Area [image: ], which should be highlighted in blue
3. In the title block, double-click in the box underneath NAME and next to DRAWN. A blank text box appears.
4. Add your name to the text box. 
5. Change the font, size, or style, in the Formatting toolbar. 
6. Click outside of the text area to save your changes. 
7. Double click in any other areas where you want to change or add text. 
8. Right-click anywhere in the drawing sheet, and select Edit Sheet to exit the edit sheet format mode. 
9. Then click on Zoom to Fit [image: ] on the View Toolbar. 
Saving the Drawing Sheet
1. Click File > Save As
2. Give your file a suitable name (If you haven’t already added a title to your drawing, the file name will automatically be used)
3. Click Save
Creating a Drawing of a Part
1. Open the Part file that you want to make a drawing of. Then return to the drawing window. 
2. Click Model View on the View Layout toolbar.
3. In the Property Manager, do the following:
a. Under Part/Assembly to Insert, double click on your part
b. For Orientation, click Front Under the Standard views
c. Select Preview to display a preview in the graphics area.
d. Under Options select Auto-start projected view
e. Under Display Style, click HiHiHidden Lines Visible
4. Move the pointer into the graphics area.
5. Click to place the front view as Drawing View 1 shown below.
6. Move the pointer up, and click to place Drawing View 2, then move to the side and click to place Drawing View 3.
7. Then click the  in the Property Manager
[image: ]
Moving Drawing Views
If you click on one of the drawings, then hover over the border around the drawing, you will then be able to click and move the drawings to the position where you want them. 
Inserting an Isometric View
1. Click on the Model View  on the View Layout toolbar
2. Double click on your part file listed
3. Under Orientation, click Isometric under the standard views
4. Under Display Style, click Shaded with Edges
5. Click on the sheet where you want to place the new view
6. Click 
Adding Dimensions to a Drawing
1. Click on the Annotation tab
2. Click on Smart Dimension
3. You can now dimension your drawing in the same way as you did during the building of your part. 
4. Make sure that you do not over define your drawing by having dimensions included more than once. 
5. Remember that all dimensions should be clear and the no numbers should be touching any lines. 
6. To dimension a chamfer, you will need to click on the drop down menu under Smart Dimension and click on Chamfer Dimension
7. Then you need to click the line that is at the angle plus the horizontal line it touches. 
To Save as a PDF
1. Remember to save the file as a drawing file first.
2. Click on File>Save As, under Save as type select Adobe Portable Document Format (*.pdf)
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