Steven Moore
Networks and Cybersecurity Essentials (ACCA4024) Lab1
1.Ipconfig What is the IP address of the computer?
192.168.1.10
2.What is the subnet mask of the computer?
255.255.255.0
3.Ping 192.168.1.11 (Other PC’s IP Address) Was the ping successful? 
Yes 4 packets sent 4 received.
4.Click PCB (PC1)  Desktop  Command Prompt  a. Ipconfig What is the IP address of the computer? 
192.168.1.11
5.What is the subnet mask of the computer?
255.255.255.0
6.Ping 192.168.1.10 (Other PC’s IP Address) Was the ping successful?  
Yes 4 packets sent 4 received.
7.Is your IP Address Automatically configured or Manually Configured?
Automatically
8.ping google Were the ping results successful? 
yes 4 packets sent / received average ping 11ms
9.Type tracert www.google.com and press Enter.
Tracing route to google over maximum of 30 hops:
1 3ms 3ms 5ms broadband.bt.com(Address)
2 5ms 7ms 5ms www.Google.com
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