Router1#show running-config
Building configuration...


Current configuration : 1303 bytes
!
! Last configuration change at 13:13:32 UTC Tue Jan 14 2020
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname Router1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$DRvi$wgE30ARtQyfph1bs5O4kb1
enable password class
!
no aaa new-model
!
no ip domain lookup
ip admission watch-list expiry-time 0
!
!
!
!
!
!
!
!
!
!
subscriber templating
multilink bundle-name authenticated
!
!
!
!
!
license udi pid ISR4221/K9 sn FGL22359289
no license smart enable
diagnostic bootup level minimal
!
spanning-tree extend system-id
!
!
!
!
redundancy
 mode none
!
!
!
!
!
!
!
!
interface GigabitEthernet0/0/0
 description Router-PC-B connection
 ip address 153.99.10.1 255.255.255.0
 negotiation auto
!
interface GigabitEthernet0/0/1
 description Router-Switch connection
 ip address 153.99.11.1 255.255.255.0
 negotiation auto
!
interface Serial0/1/0
 no ip address
!
interface Serial0/1/1
 no ip address
!
ip forward-protocol nd
no ip http server
ip http secure-server
!
!
!
!
!
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