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This document I will be my Task 3 for my exam.


Task3: Network connectivity (10 marks)

Using ping command, verify end-to-end connectivity:
From PC-1, ping PC-2 & LP-A. Is it successful? 			yes			 From PC-1, ping default gateway. Is it successful? 			yes				 From PC-2, ping 172.16.0.1. Is it successful? 	yes	 From PC-1, ping 172.16.0.254. Is it successful? 		no		


Verify HSRP is working as expected
Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-2, ping 172.16.0.1. Ping should not be successful 	no	 From PC-2, ping default gateway. Is it successful? 	no		  From PC-2, ping 209.165.200.225. Is it successful? 		no			

