Revision 1
Q1
(i) Determine the reduced state diagram for the state diagram given below.
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(ii) For the Obtained reduced state diagram
(a) [bookmark: _Hlk129365770]Show its state Assignment.						     
(b) Obtain the State Table.                                                                                 
(c) Obtain Excitation Table using any Flip- flop.			
(d) [bookmark: _Hlk129367624]Output Expressions 							
(e) Logic Circuit		
Q2
(i) Determine the reduced state diagram for the state diagram given below.
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(ii) For the Obtained reduced state diagram
(a) Show its state Assignment.						     
(b) Obtain the State Table.                                                                                 
(c) Obtain Excitation Table using any Flip- flop.			
(d) Output Expressions 							
Logic Circuit								

Q3
(i) Design a Synchronous Circuit for the Sequence Detector that produces an output ‘1’ whenever the non-over lapping sequence 1011 is detected. Also Represent the following.	
(a) State Diagram.							
(b) Present state, Next state, output Table.				
(c) Excitation Table.							
(d) Simplified K- Map Expression.					
(e) Logic Diagram.																
Q4
(ii) Design a Synchronous Circuit for the Sequence Detector that produces an output ‘1’ whenever the non-over lapping sequence 1100 is detected. Also Represent the following.	
(f) State Diagram.							
(g) Present state, Next state, output Table.				
(h) Excitation Table.							
(i) Simplified K- Map Expression.					
(j) Logic Diagram.	
Q5
(i) Design a Mod 6 counter using J-K flipflop for an asynchronous Sequential Circuit. Answer the following
(a) State Diagram							
(b)  State Table								
(c) State Assignment							
(d) Excitation Table							
(e) Simplified Expressions using K- Map				
(f) Logic Design.				
Q6
(i) Design a Mod 5 counter using J-K flipflop for an asynchronous Sequential Circuit. Answer the following
(a) State Diagram							
(b)  State Table								
(c) State Assignment							
(d) Excitation Table							
(e) Simplified Expressions using K- Map				
(f) Logic Design.								
							
					
Q7
For the JK – flipflop and D Flipflop , answer the following
(a) Characteristic Equation
(b) State Table
(c) Excitation Table
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