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Ms     ( to be found prior to test )
Musf =  38 kg /wheel   
Musr =   42 kg/wheel  	
CG height for sprung mass to be determined in Test 1 and compared with the workshop value.
Wheelbase 	2.351m	
Rolling radius 0.275 m  for Avon Radial Slicks ( NB this is nominal figure – each tyre type  will be slightly different )
Front spring rate left 55.62 N/mm   Right 57.49 N/mm 
Rear spring rate 170 lb/in
Ratio of  wheel  travel to spring travel  1.97
Ratio of  wheel  travel to pot travel   1.622
Rear Suspension leverage of wheel to spring = 1.0
Velocity  ratio of damper wheel to pot  = 1.0	
Roll centre heights  and track to be found in WinGeo3 models 
	 

