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	Personnel Involved:

Personnel in the immediate location.
	PPE: All personnel will wear hard hats, safety footwear and high visibility jackets/vest and gloves 
	SUPERVISOR IN CHARGE: 
C Keys

	Operation: Formwork

	ACTIVITY AND HAZARDS

(Identify hazards associated with task)
	INITIAL RISK RATING
	CONTROL MEASURES

(Identify measures to eliminate, reduce or control hazard or those that are requested by others)
	RESIDUAL RISK RATING
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	Manuel Handling

Use of Power tools

Use of hand tools

Cuts and abrasion

Trips and falls

Working in excavations

Use of mould oils

Effects on environment
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Task, Individual, Load, Environment, should all be considered before any lifting 

Where practicable shutters to be lifted into place using an excavator.

Unload Materials as close to work area as practical.

Split bundles/packs to reduce weight to be carried by operatives.

All lifting will be controlled by a banks man  

All power tools to be 110v and hold current PAT test 

All tools to be fit for purpose and be inspected daily prior to use

Results of inspection to be recorded in site file.

Eye and ear protection to be worn when using power tools.

Keep work area tidy and free of debris

All tools to be fit for purpose and be inspected daily prior to use

Results of inspection to be recorded in site file.

Eye and ear protection to be worn when using power tools.

Gloves to be worn when oiling shutters.

Eye and ear protection to be worn when using power tools.

All tools to be fit for purpose and be inspected daily prior to use

Results of inspection to be recorded in site file.

Keep work area tidy and free of debris

All power tools to be 110v and hold current PAT test 

Keep work area tidy and free of debris

Prefabrication to be in designated work area.

Where practicable shutters to be lifted into place using an excavator.

Gloves to be worn when oiling shutters.

Where possible Dancourt ltd will endeavour to use timber from a sustainable source.


	(
(
(
(
(
(
(
(

	
	


All persons undertaking activities indicated on this risk assessment form must be made fully aware of its contents
