
Method to find Centre of Gravity Position 



Use corner weight scales to find F1 and R1  and hence X on diagram

				
Lift front of vehicle so that front wheels are at height h and re - weigh to find F2 and R2

 (
h
)

The height (Y) of the centre of Gravity of the total mass can then be found from the following relationship.


			    

The CG of the unsprung mass is taken as acting at wheel centre height The height of the CG of the sprung mass is found by taking horizontal moments about one road/  tyre contact point. 
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