Imran Ali 1701017

Cardiff Router

User Access Verification

Password: 

Cardiff>en
Password: 
Cardiff#sh ru
Cardiff#sh running-config 
Building configuration...

Current configuration : 1589 bytes
!
version 15.1
no service timestamps log datetime msec
no service timestamps debug datetime msec
service password-encryption
!
hostname Cardiff
!
!
!
enable secret 5 $1$mERr$9cTjUIEqNGurQiFU.ZeCi1
!
!
ip dhcp excluded-address 172.16.198.1 172.16.198.5
!
ip dhcp pool CardifFDHCP
network 172.16.198.0 255.255.255.192
default-router 172.16.198.1
dns-server 172.16.198.1
!
!
!
no ip cef
no ipv6 cef
!
!
!
username admin password 7 0822455D0A16
username cardiff password 7 08364D400C01041A405B5E54
!
!
license udi pid CISCO2901/K9 sn FTX1524J6F6-
!
!
!
!
!
!
!
!
!
no ip domain-lookup
ip domain-name wanexam2020.com
!
!
spanning-tree mode pvst
!
!
!
!
!
!
interface Tunnel10
ip address 192.168.10.1 255.255.255.248
mtu 1476
tunnel source Serial0/3/0
tunnel destination 10.0.1.225
!
!
interface GigabitEthernet0/0
no ip address
duplex auto
speed auto
!
interface GigabitEthernet0/1
ip address 172.16.198.1 255.255.255.192
duplex auto
speed auto
!
interface Serial0/3/0
ip address 10.0.1.22 255.255.255.252
encapsulation ppp
ppp authentication chap
clock rate 2000000
!
interface Serial0/3/1
no ip address
encapsulation ppp
clock rate 2000000
shutdown
!
interface Vlan1
no ip address
shutdown
!
router bgp 65025
bgp log-neighbor-changes
no synchronization
network 10.0.0.0
network 10.0.1.20 mask 255.255.255.252
!
ip classless
ip route 0.0.0.0 0.0.0.0 209.165.201.253 
!
ip flow-export version 9
!
!
!
!
!
!
!
!
line con 0
password 7 0822455D0A16
logging synchronous
login
!
line aux 0
!
line vty 0 4
password 7 0822455D0A16
login
transport input ssh
!
!
!
end



