Labs 1 Work 
7.a.
What is the IP address of the computer? 
192.168.1.10
What is the subnet mask of the computer? 
 255.255.255.0

7.b.	Ping 192.168.1.11 (Other PC’s IP Address) Was the ping successful?  
What is the IP address of the computer? 
 192.168.1.11
What is the subnet mask of the computer? 
 255.255.255.0

Task 2
step - 5. Automatically 
Were the ping results successful? Yes
Pinging www.google.com [216.58.212.228] with 32 bytes of data:
Reply from 216.58.212.228: bytes=32 time=9ms TTL=120
Reply from 216.58.212.228: bytes=32 time=8ms TTL=120
Reply from 216.58.212.228: bytes=32 time=8ms TTL=120
Reply from 216.58.212.228: bytes=32 time=7ms TTL=120
Ping statistics for 216.58.212.228:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 7ms, Maximum = 9ms, Average = 8ms

step - 6. 
C:\Users\ashle>tracert www.google.com

Tracing route to www.google.com [216.58.212.228]
over a maximum of 30 hops:

  1    <1 ms    <1 ms     2 ms  192.168.128.1
  2    14 ms    16 ms    17 ms  no-dns-yet.as25178.net [109.246.19.181]
  3     7 ms     7 ms     7 ms  no-dns-yet.as25178.net [109.246.30.8]
  4    11 ms     7 ms     7 ms  72.14.195.60
  5     8 ms     9 ms     8 ms  108.170.246.161
  6     8 ms     8 ms     8 ms  216.239.41.241
  7     7 ms     7 ms     7 ms  lhr25s28-in-f4.1e100.net [216.58.212.228]

Trace complete.

Reflection/ Summary 

After this first labs lecture I now have a basic understanding on how to use Packet Tracer
and how it can be used in many different ways to check and simulate different systems. 
I was able to follow allong with the Labs Tutorial quite well however some of the material 
I was unable to identically follow as of the no ethernet connection. Regardless of this 
I was still able to complete the command prompt tasks and everything worked successfully 
and gave me the results and answers that I have above.
