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Network and cybersecurity essentials 
Lab 1

a. Ipconfig 
What is the IP address of the computer? 
192.169.1.10
----------------------------------------------------- 
What is the subnet mask of the computer? 
255.255.255.0
------------------------------------------------------ 
b. Ping 192.168.1.11 (Other PC’s IP Address) 

Was the ping successful? 
Yes
------------------------------------------------------- 
8. Click PCB (PC1)  Desktop  Command Prompt  a. Ipconfig 

What is the IP address of the computer? 
192.168.1.11
----------------------------------------------------- 
What is the subnet mask of the computer? 
255.255.255.0
------------------------------------------------------ 
b. Ping 192.168.1.10 (Other PC’s IP Address) 

Was the ping successful? 
Yes

Automated configuration 

Yes the ping to www.google.com was successful 
The Traceroute function assists with diagnosing connectivity issues through the network. It was interesting to see where my data traffic travels through the network and the passing points in which data is sent back to my PC. Netacad is a great tool for modelling and testing network topology.
