Task3: Network connectivity (10 marks)

Using ping command, verify end-to-end connectivity:
From PC-1, ping PC-2 & LP-A. Is it successful? 		no			 From PC-1, ping default gateway. Is it successful? 			yes				 From PC-2, ping 
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172.16.0.1. Is it successful? 	no	 From PC-1, ping 172.16.0.254. Is it successful? 		yes		
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Verify HSRP is working as expected
Issue the shutdown command on R1 G0/1, and then re-issue the following commands to verify that HSRP is working as expected:
From PC-2, ping 172.16.0.1. Ping should not be successful 	no	
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 From PC-2, ping default gateway. Is it successful? 	yes		 






 From PC-2, ping 209.165.200.225. Is it successful? 	no			
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Pinging 192.168.1.1 with 32 bytes of data:

Reply from 192.168.1.1 TTI=255
Reply from 192.168.1.1: TTL=255
Reply from 192.168.1.1 TTL=255
Reply from 192.168.1.1 TTL=255

Ping statistics for 192.168.1.1
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),

Approximate round trip times in milli-second:
Minimm = Oms, Maximum = Oms, Average

oms
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C:\>ping 172.16.0.254
Pinging 172.16.0.25¢ with 32 bytes of data:

Request timed out.
Request timed out.
Reply from 172.16.0.254:
‘lleply from 172.16.0.254:
Ping statistics for 172.16.0.254:

Packets: Sent = 4, Received = 2, Lost = 2 (50% loss),
Approximate round trip times in milli-seconds:

Minimum = Oms, Maximum = 10ms, Average = Sms

2 time<lms TTL=126
2 time=l0ms TTL=126

c:\>
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ing statistics for 172.16.0.
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

\>ping 172.16.0.1

inging 172.16.0.1 with 32 bytes of dat:

equest timed out.
equest timed out.
equest timed out.
equest timed out.

ing statistics for 172.16.0.
Packets: Sent = 4, Received = 0, Lost = 4 (100% loss),

>
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C:\>ping 172.16.0.3
Pinging 172.16.0.3 with 32 bytes of data:

time<ims TTL=255
time=6ms TTL=255
time<ims TTL=255
time<ims TTL=255

Reply from 172.16.0.
Reply from 172.16.0.
Reply from 172.16.0.
Reply from 172.16.0.

Ping statistics for 172.16.0.3:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimm = Oms, Maximum = 6ms, Average = lms
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