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	Construction Method Statement
	Caretakers House


Fixing Porch Roof
	Step
	Significant Hazards 
	Risks 
	Existing Control Measure 
	Additional Recommendations 

	Arrival on Site

	Slips trips and falls
	LOW
	Sign site register 
Complete toolbox talks and site progress meetings for update on site. 
	Correct PPE to be worn 

	Work at height register

	Slips trips and falls
	LOW
	Read risk Assessments and method statements.
Sign working at height register.
Ensure all tools, equipment and materials are available prior to starting to avoid leaving the area unattended. Check scaffolding is at the correct height and check Scaff-tags. 
	Correct PPE to be worn
All power tool protection to be used. 

	Materials delivered to site and delivered to working area. 

	Pedestrians, manual handling, use of machinery, tip hazards. 
	MED 
	Use of mechanical lifting where practically possible. 
Ground conditions to be level and free from debris.
All waste to be disposed of at regular intervals and working areas kept clean.

	Correct PPE to be worn. 
Use of ladders to be class 1 and checked and used on level ground. 

	Storage of materials

	Working area being overcrowded, materials falling, damage to materials, manual handling, trip hazards. 
	MED
	Delivery of materials to be stored correctly and checked for damage. 
Materials stored in the correct areas to avoid damage. 
	Manual Handling procedures carried out correctly and where practically possible use of mechanical lifting aids used. 

	Fixing of wall plate and trusses
	Falls from height, manual handling, falling objects. 
	MED 
	Restrict operatives working in the area and any access needed to the building will need to be sealed off and alternative access used. 
Correct use of scaffolding used and checked before us. 
All tools and materials to be in place and checked before work commences. Area not to be left unsupervised if tools and equipment is left out. 
	Manual Handling procedures carried out correctly and where practically possible use of mechanical lifting aids used. Correct PPE to be worn
All power tool protection to be used

	Clean up

	Manual handling, dust.

	MED 
	All waste and debris to be removed and whilst complying with waste management plan. 
	PPE to be worn at all times. 

	Completion

	Slips trips and falls 
	LOW
	Inform Site manager of completion. 
	PPE to be worn at all times





	
