	Device
	Issue
	Action

	Branch-2 
	Ip address incorrect on serial interface
	Changed to 192.168.0.6

	PC5
	Incorrect default gateway
	Change PC gateway to 192.168.5.129

	Hub 
	Missing nat configuration on s0/1/0
	added ip nat inside to serial interface s0/1/0

	Factory 
	Network interface was down
	Ran no shut down command on network interface

	Factory
	Network entry missing from OSPF config on router
	Ran the following :-
Router ospf 10
Network 192.168.4.0 0.0.0.255 area 0



