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TASK 1 
References (Configuring IPv6 Address) Practice the below commands with the above topology.  
 	Manual Configuration 
 	 	R1 Gi0/0/1 	ipv6 address 2003::1/64 
 	 	R2 Gi0/0/1 	ipv6 address 2003::2/64 
 	EUI – 64 Configuration 
 	 	R1 Gi0/0/0 	ipv6 address 2001:: /64 eui-64 
 	 	R4 Gi0/0/0 	ipv6 address 2001:: /64 eui-64 
GigabitEthernet0/0/0 [up/up] FE80::2D0:97FF:FE90:5701 
2001::2D0:97FF:FE90:5701 
 	EUI – 64 Configuration with Link Local 
R3 Gi0/0/1 ipv6 address 2002:: /64 eui-64  ┘ fe80::1 Link Local   R4 Gi0/0/1 ipv6 address 2002:: /64 eui-64  ┘ fe80::2 Link Local 
GigabitEthernet0/0/1 [up/up] 
FE80::1 
2002::1 
GigabitEthernet0/0/1 [up/up] 
FE80::2 
2002::2 
 	Auto Configuration 
	R3 Gi0/0/0 	ipv6 address 2000:: 2/64 eui-64  ┘  
 	 	R2 Gi0/0/0 	ipv6 address Autoconfig eui-64  ┘  
GigabitEthernet0/0/0 [up/up] 
FE80::260:47FF:FE8A:E01 
2000::2 
 	Other Commands 
Show interface gi0/0/0 
Show ipv6 interface brief 
Show ipv6 interface brief 
Debug ipv6 nd 
Debug ipv6 packets 
Ping 
 
Configuring Static IPv6 Route 
 Ipv6 route ipaddr (1111::/16 or /64 as per scenario) Next hop ip addres 2000:12::1 
 Ipv6 route ipaddr (::/0) Next hop ip addres 2000:12::1 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
TASK 2 
Design this Topology and Configure IPv4 and IPv6 Addresses as per the description below (image) and configure Static/ Default routes to establish communication successfully. 
 
[image: ] 
TASK 3 
Complete the two PKA Files (Available in Moodle and Teams) 
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