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Incorrect Prefix
Reconfigure with  .128
Static Route for LAN1 Incorrect
R2

Reconfigure with   2001:DB8:1::/64
Reconfigure with  172.31.1.198  
IPv4 Address incorrect
R2

Reconfigure with   172.31.1.194
IPv4 Address incorrect
R2

Reconfigure with 172.31.1.193  
Next hop IP inccorect
R1
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