Tutorial 3
1. Design the state diagram for a 4 bit counter, that counts from sequentially 0000 to 1111 when signal S is asserted and holds its count when signal S is de-asserted.

2. Design the state diagram only for a circuit that counts 0, 2, 5, 6 continually if an input I = 1 but counts 0, 1, 3, 4, 7 continually if I=0. If I changes in the middle of a sequence then the circuit will return to 0 first and continue on the new count sequence.

3. 
a) Identify the class of FSM shown below.
b) Generate the expressions for each of the d flip-flop inputs.
c) Generate a present/next state map for the circuit.
d) Develop a state diagram to graphically illustrate the circuit’s state to state behaviour.
e) Is there a problem with this circuit, if so what is it?
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4.          Consider the finite state machine represented by the state diagram below and design a VHDL behavioral model for this system.
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