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Objectives 

Using Packet Capturing tools and network monitoring tools.  
Tasks 

1. Use Nmap to scan 2.  
Required Resources 

· PC with Ubuntu 16.0.4 LTS installed in a VirtualBox or VMware virtual machine. (Alternatively, Any Linux Platform) 
· Internet Connection to refer the outcomes o References: https://nmap.org/ 
 
Task 1 

· Login as User Cisco. 
· Go to Terminal and Type the following commands and examine  o To do that we are using Nmap.  
 Network Mapper, or Nmap, is an open source utility used for network discovery and security auditing. Administrators also use Nmap for monitoring hosts or managing service upgrade schedules.   Nmap determines  
· what hosts are available on a network,  
· what services are running,  
· what operating systems are running,  • What packet filters or firewalls are running? 
o So, basically if you could get all the above details using Nmap, you could get few information which could be used later in performing attacks or mitigating attacks.  
 
 
 
 
 
 
 
 
 
 
 
 
· Commands to execute o Step 1: 
 nmap localhost 
(This is a scan performed to get information about the services that are bound to the localhost) 
	 
 Starting Nmap 7.01 ( https://nmap.org ) at 2020-12-19 09:32 CST
Nmap scan report for localhost (127.0.0.1)
Host is up (0.000052s latency).
Not shown: 997 closed ports
PORT    STATE SERVICE
22/tcp  open  ssh
23/tcp  open  telnet
631/tcp open  ipp
 
 
 
 


 
o Step 2: 
 Replace the above command with your IP Address and other hosts (if connected/ else ignore) in your network to check the outcomes. 
Type the command you used to find out your host IP Address 
ifconfig  
Type the command you used to scan after finding your host IP Address 
-nmap 127.0.0.1 
Record the outcomes of the above command here
Starting Nmap 7.01 ( https://nmap.org ) at 2020-12-19 09:35 CST
Nmap scan report for localhost (127.0.0.1)
Host is up (0.000068s latency).
Not shown: 997 closed ports
PORT    STATE SERVICE
22/tcp  open  ssh
23/tcp  open  telnet
631/tcp open  ipp

Nmap done: 1 IP address (1 host up) scanned in 0.08 second 
 
 
 
 
 o Step 3: Analyse the outputs/outcomes from Step 1 and 2 and record your reflections. (Hint: Analyse what is the difference between local host and ip address of the host, If ports displayed are different, Why is it different? etc (not limited to the hints)) 
	 The ports came out the same, the difference was mostly in the scan speed 
 
 
 


· Step 4: Why is the nmap scan only scans the first 1000 ports? What will be the command to scan all the ports? 
	 Because that is the default number of ports to scan, to scan more you would need to use the command: nmap –p– host 

 
 


 
· Step 5: Scan the UDP Ports 
· nmap –sU localhost 
(This is a scan performed to get information about the UDP ports and to execute this command you need root privileges. So, try) 
· sudo nmap –sU localhost 
Record the outcomes of the above command here (Hint: what UDP ports could you find open through your scan) 
 
Starting Nmap 7.01 ( https://nmap.org ) at 2020-12-19 09:48 CST
Failed to resolve "–sU".
Nmap scan report for localhost (127.0.0.1)
Host is up (0.0000080s latency).
Not shown: 997 closed ports
PORT    STATE SERVICE
22/tcp  open  ssh
23/tcp  open  telnet
631/tcp open  ipp

Nmap done: 1 IP address (1 host up) scanned in 1.64 seconds
cisco@ubuntu:~$  7.01 ( https://nmap.org ) at 2020-12-19 09:48 CST
bash: syntax error near unexpected token `https://nmap.org'
cisco@ubuntu:~$ Failed to resolve "–sU".
Failed: command not found
cisco@ubuntu:~$ Nmap scan report for localhost (127.0.0.1)
bash: syntax error near unexpected token `('
cisco@ubuntu:~$ Host is up (0.0000080s latency).
bash: syntax error near unexpected token `('
cisco@ubuntu:~$ Not shown: 997 closed ports
No command 'Not' found, did you mean:
 Command 'jot' from package 'athena-jot' (universe)
 Command 'hot' from package 'hopenpgp-tools' (universe)
 Command 'dot' from package 'graphviz' (main)
Not: command not found
cisco@ubuntu:~$ PORT    STATE SERVICE
PORT: command not found
cisco@ubuntu:~$ 22/tcp  open  ssh
bash: 22/tcp: No such file or directory
cisco@ubuntu:~$ 23/tcp  open  telnet
bash: 23/tcp: No such file or directory
cisco@ubuntu:~$ 631/tcp open  ipp
bash: 631/tcp: No such file or directory
cisco@ubuntu:~$ 
cisco@ubuntu:~$ Nmap done: 1 IP address (1 host up) scanned in 1.64 seconds
 
 
· Step 6: From the above outcomes select any ports which is open 
 sudo nmap –p137 localhost  
(Change the port number 137 to any port which you found as open in the previous step (5).) 
Record the outcomes of the above command here (Hint: Is the port open or closed? Why? Also, record the use of –p command) 
The port is open, because it is not protected. -p637
 
· Step 7: Try other port related commands and record its purpose. 
· sudo nmap –pportnumber host_ip 
· sudo nmap –pportnumber_startrange-portnumber_endrange host_ip 
· sudo nmap –pportnumber,portnumber host_ip 
· not limited to the above (Do a google search, refine your search and find out other port related commands, Hint:nmap.org) 
Record the outcomes of the above commands here  
 Scans a specific port on a host, scans a range of ports on a host, scans multiple ports on a host
 
 
 
 
· Step 8: Detecting the version is a very important part of information gathering. Try to find out the version.  nmap –sV localhost  
Record the outcomes of the above commands here  

Starting Nmap 7.01 ( https://nmap.org ) at 2020-12-19 09:55 CST
Failed to resolve "–sV".
Nmap scan report for localhost (127.0.0.1)
Host is up (0.000052s latency).
Not shown: 997 closed ports
PORT    STATE SERVICE
22/tcp  open  ssh
23/tcp  open  telnet
631/tcp open  ipp

Nmap done: 1 IP address (1 host up) scanned in 0.17 seconds
 
 
 
 
 
 
 
· Step 9: Try other commands to detect other versions and record its purpose. 
· Command to identify the Operating System version 
Record the outcomes of the above commands here 
 
 
 
 
 
 
 
· Command to identify the Service Version 
Record the outcomes of the above commands here 
 
 
 
 
 
 
Learnings from tutorials so far:  
Part 1 (Packet Tracer, Host Machines) 
· Build a home Network  
· Understand and configure IP Address 
· Use Ping/ Trace route Utility to check the connection status 
· Use ipconfig /all command to determine the MAC address of a Windows computer on an Ethernet network. 
· Analyze a MAC address to determine the manufacturer. 
· Analyze the Wired and Wireless Network connection. 
· Analyze Address Resolution Protocol (ARP). 
· Connect to a Wireless Router and configure the basic settings in a wireless router and add security features. 
· Use nslookup command to understand the url to ip conversion. 
· Configure basic connectivity settings in Intermediate devices (Switch/ Router). 
· Work with SBA Packet Tracer Files/ environment 
· Configure ftp, web, email, dns, ntp and aaa Servers Part 2 
· Set up a virtual lab environment  
· Troubleshooting the virtual lab environment 
· Working with virtual machines 
· Authentication, Authorization and Accounting 
· Threats and Vulnerabilities – Using NMAP 

	2 	n.kaliyamurthy@uwtsd.ac.uk                                                                                                           
 
	2 	n.kaliyamurthy@uwtsd.ac.uk                                                                                                           
 
image1.jpg
PRIFYSGOL CYMRU
Y Drindod Dewi Sant
UNIVERSITY OF WALES

Trinity Saint David

SWANSEA - ABERTAWE




image2.png
Cisco | Networking Academy®
Mind Wide Open”




