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Lab: IPv4, Subnetting, VLSM and IPv6 Addressing


Understanding IPv4 and IPv6 addressing (word count 1000) 
This part of lab worksheet require you research and write a report on “Features of IPv6”. You may discuss but not limited to structure, address types, advanced functionalities and security.  
Subnetting and VLSM

NOTE: To complete this part you would need full understanding of Lab 10 to 14. 
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Using the Network address 172.16.2.0/24, VLSM the network to support the following requirements: 
Subnet A: 16 hosts/27   
Subnet B: 2000 hosts/21
Subnet C: 6 hosts/29
Subnet D: 500 hosts/23
Subnet E: 60 hosts/26
Subnet F: 180 hosts and Serial links between routers/24
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Table 1
	Subnet
	Network Address
	Subnet mask
	First Address
	Last Address
	Broadcast Address

	B
	172.16.2.0/21
	255.255.248.0
	172.16.2.1
	172.16.9.254
	172.16.9.255

	D
	172.16.10.0/23
	255.255.254.0
	172.16.10.1
	172.16.11.254
	172.16.11.255

	F
	172.16.12.0/24
	255.255.255.0
	172.16.12.1
	172.16.12.6
	172.16.12.7

	E
	172.16.13.0/26
	255.255.255.192
	172.16.13.1
	172.16.13.62
	172.16.13.63

	A
	172.16.13.64/27
	255.255.255.224
	172.16.13.65
	172.16.13.94
	172.16.13.95

	C
	172.16.13.96/29
	255.255.255.248
	172.16.13.97
	172.16.13.102
	172.16.13.103

	R1-R2
	172.16.13.104/30
	255.255.255.252
	172.16.13.105
	172.16.13.106
	172.16.13.107

	R2-R3
	172.16.13.108/30
	255.255.255.252
	172.16.13.109
	172.16.13.110
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