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IATG SAFERGUARD TRAINING MODULES
MODULE MA04 – QUANTITY DISTANCES (IATG 02:20) – EXERCISE 1
MINI-EXERCISE
SCENARIO

You have just been offered use of a small ammunition storage facility. 

The facility includes 3 x ESH, numbered 1 to 3.  There are no other structures within this facility.  

· ESH 1 is a light structure. 

· ESH 2 is a heavy walled building with a reinforced roof.  It has a manmade traverse on one side, and a significant ground feature, which constitutes a natural traverse to another.  

· ESH 3 is a light structure.

The nearest inhabited building outside the perimeter is a residential house which your troops use for accommodation and an office.   It should be treated as an ‘inhabited building’.  

There are no other houses, nor are there any vulnerable sites.  There is no real road in the area.  

DATA

Distances (in meters): 

	Location
	ESH 1
	ESH 2
	ESH 3
	HOUSE

	ESH 1
	N/A
	
	
	

	ESH 2
	100m
	N/A
	
	

	ESH 3
	200m
	260m
	N/A
	

	HOUSE
	450m
	500m
	150m
	N/A


Ammunition Storage Requirements:
You have a quantity of HD 1.1D.  You are directed that this must only go into a traversed ESH as it is a battle-winning nature.   This means that all the HD ammunition must go into ESH 2.  
You have a quantity of HD 1.3.1G, which you are directed must be stored on its own due to the Compatibility Group ‘G’.  You decide to store this stock in ESH 1.  

You have a large quantity of 1.4S ammunition (small arms ammunition).  You decide this should be stored in ESH 3.  

Your boss has told you that a “limited degree of protection” is acceptable for all stocks. 

QUESTIONS

1.
What is the maximum NEQ of Hazard Division 1.1 that may be stored in ESH 2?  

a. Max NEQ based on distance to ESH 1:
b. Max NEQ based on distance to ESH 3:
c. Max NEQ based on distance to Inhabited Building: 
d. Therefore - maximum permissible NEQ if HD 1.1 to be stored in ESH 2: 
2.
What is the maximum NEQ of Hazard Division 1.3.1 that may be stored in ESH 1?  

3.
What is the maximum NEQ of Hazard Division 1.4 that may be stored in ESH 3?

(Hint – think about what you were taught about HD 1.4 and the distances to be applied!)
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