	S1#show run
S1#show running-config
Building configuration...

Current configuration : 1521 bytes
!
! Last configuration change at 05:42:15 UTC Mon Mar 8 1993
!
version 15.2
no service pad
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
!
hostname S1
!
boot-start-marker
boot-end-marker
!
enable secret 5 $1$j5nA$DdSj.grOJKTZc3Xys7POk0
enable password 7 0822404F1A0A
!
no aaa new-model
system mtu routing 1500
!
!
 --More--


S1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
Vlan1                  172.16.11.10    YES manual up                    up
FastEthernet0/1        unassigned      YES unset  down                  down
FastEthernet0/2        unassigned      YES unset  down                  down
FastEthernet0/3        unassigned      YES unset  down                  down
FastEthernet0/4        unassigned      YES unset  down                  down
FastEthernet0/5        unassigned      YES unset  up                    up
FastEthernet0/6        unassigned      YES unset  up                    up
FastEthernet0/7        unassigned      YES unset  down                  down
FastEthernet0/8        unassigned      YES unset  down                  down
FastEthernet0/9        unassigned      YES unset  down                  down
FastEthernet0/10       unassigned      YES unset  down                  down
FastEthernet0/11       unassigned      YES unset  down                  down
FastEthernet0/12       unassigned      YES unset  down                  down
FastEthernet0/13       unassigned      YES unset  down                  down
FastEthernet0/14       unassigned      YES unset  down                  down
FastEthernet0/15       unassigned      YES unset  down                  down
FastEthernet0/16       unassigned      YES unset  down                  down
FastEthernet0/17       unassigned      YES unset  down                  down
FastEthernet0/18       unassigned      YES unset  down                  down
FastEthernet0/19       unassigned      YES unset  down                  down
FastEthernet0/20       unassigned      YES unset  down                  down
 --More--






C:\Users\Admin>ping 172.16.10.254

Pinging 172.16.10.254 with 32 bytes of data:
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127
Reply from 172.16.10.254: bytes=32 time<1ms TTL=127

Ping statistics for 172.16.10.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 0ms, Average = 0ms

C:\Users\Admin>






Current configuration : 3651 bytes
!
! Last configuration change at 20:14:39 UTC Mon Apr 1 2013
!
version 16.9
service timestamps debug datetime msec
service timestamps log datetime msec
service password-encryption
platform qfp utilization monitor load 80
no platform punt-keepalive disable-kernel-core
!
hostname R1
!
boot-start-marker
boot-end-marker
!
!
enable secret 5 $1$7zoC$A.5S8q4k/kaKHsH8iJ73p1
enable password 7 045807071C32
!
no aaa new-model
!
 --More—

R1#show ip int brief
Interface              IP-Address      OK? Method Status                Protocol
GigabitEthernet0/0/0   172.16.10.1     YES manual up                    up
GigabitEthernet0/0/1   172.16.11.1     YES manual up                    up
Serial0/1/0            unassigned      YES unset  down                  down
Serial0/1/1            unassigned      YES unset  down                  down
R1#
C:\Users\Admin>ping 172.16.11.254

Pinging 172.16.11.254 with 32 bytes of data:
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127
Reply from 172.16.11.254: bytes=32 time<1ms TTL=127

Ping statistics for 172.16.11.254:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 0ms, Maximum = 0ms, Average = 0ms

C:\Users\Admin>
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