Table 1. Risk assessment: Test pitting Llanllyr site
	Activity and hazard
	Who may be harmed
	Can the risk be avoided?
	How can the risk be reduced?

	Vehicle movements
	
	
	

	Vehicle to vehicle incident (impact, crushing, fire)
	Site personnel
	No
	Keep vehicle speed and movement to a minimum and use agreed access routes

	Vehicle to pedestrian incident
	Site personnel
	No
	

	Excavation of test pits
	
	
	

	Manual handling (strain related injuries)
	Student
	Yes
	Share loads, avoid twisting where possible, use appropriate PPE such as gloves.  Follow instructions on best practice

	Exposure to contaminated sediment/water(poisoning, Weils disease)
	Student/staff
	No
	Wear gloves. Wash hands and arms prior to eating, drinking and smoking.  Keep cuts and grazes covered.  Maintain first aid kit on the site to treat breaks in skin.  First aid kit to include eye washing equipment.

	Work next to surface water (risk of drowning, risk of exposure/hypothermia)
	Student/staff
	Yes
	Works will not be carried out within 10m of deep surface water features such as filter ponds, rivers or lakes.

	
	
	
	

	Trips/falls
	Student/staff
	Yes
	Ensure tools are safely placed, take care at the edge of test pits, ensure test pits are cordoned off outside work hours.

	
	
	
	

	
	
	
	

	
	
	
	


