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1.0 Introduction 
This report is focusing on the inclusions and exclusions of the cost plan that has been compiled for the Y Fforwn Building on the UWTSD SA1 campus, Swansea. The below points have been based on the drawings that have been provided as part of the assignment. Each of the below sections will indicate where an assumption has been made. The cost plan has been complied using figures from ‘SPON'S ARCHITECTS' AND BUILDERS' PRICE BOOK 2022’. Each item has been referenced I the notes section of the cost plan. 

2.0 Assumptions 
The following assumptions have been made: 
Substructure 
· Rate of the supply and install of concrete piles has been based on 600mm dia reinforced concrete CFA piles as there is no rate for 500mm. 

· Pile Caps size are assumed at 900 mm × 900 mm × 1000 mm; 1–2 piles. This assumption has been made due to their being insufficient information of the drawings and lack of substructure detail. 

Superstructure 

· Column meterage rate has been calculated at 8.2lm x 36. This has been calculated based on a ceiling height of 3.6m per floor multiplied by the 36 columns. 

· Due to insufficient design information, I have assumed that the roof is constructed using trusses at 600mm centres. This price can be amended on receipt of a more detailed specification. 

· I have assumed that the aluminium sheet roof is applied to ply sheathing sub straight. This assumption is made on the basis that the aluminium sheeting would need to be applied to a base, however the detail is not specified in the specification. 

· The roof has been priced based on a timber trussed roof design. Despite the actual design being a cut roof, there was not an accurate rate in Spons based on this design, so the next best alternative was selected. 

· An allowance has been made for trims and flashings of 5 percent of the overall cost of the roof. Given the design of the roof and size, I deemed a 5 percent allowance was acceptable to cover the cost of flashing and trims. 

· I have based the cost of the PV solar panels on the residential cost as this is the only cost that is available through using Spons. 

· I have assumed that the vinyl flooring is the same throughout the whole building. There is no specification to detail various designs, so it is assumed they are all the same specification. 

· I have assumed that the carpet as ' Carpet tiles; including underlay, edge grippers heavy domestic duty' is the same throughout the whole building. There is no specification to detail various designs, so it is assumed they are all the same specification.

· I have not provided a cost for ceiling finishes due to the ceiling in the library block having a concrete board finish. It is there fore assumed that a finish cost is not required. 

· As there is no specification, I have assumed that the wall finishes are a standard one miss coat and two coats of emulsion to both the internal and external skins as this is standard throughout buildings of this nature. 

External Works 

· No costs have been allocated for the following external works due to their being in sufficient information to provide an accurate price: 
· Site Preparation 
· Roads, Paths, paving’s and surfacing
· Soft landscapes, planting and irrigation systems
· Fencing, railings and walls
· External Drainage
· External Services

· I have assumed a meterage of 250m for the connection of external services due to insufficient information on the drawings, I have deemed this the most appropriate rate, the distance from the existing mains supply has been estimated.

· I have assumed the street lighting will be based on the same specification as an estate road area on an assumption that there will be 50 columns.


General Notes 
· Due to the Corona Virus pandemic and the increased cost of materials, I have assumed all costs taken from spoons are of the highest rate.
· Items that have been deemed as not applicable have been marked on the cost plan. 


Conclusion 
The cost plan for the Y Fforwm Building has been based on the drawings available. Should more information become available, the costs can be revised accordingly. The rates taken from Spons are not relevant to the location of the build, this may alter the final cost when the location is taken into consideration. 
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