How to  Plot Velocity of Bullet in ABAQUS:

IN VISUALIZER:
Make sure plane cut is switched off, SELECT CREATE XY DATA:
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Select ODB FIELD OUTPUT:
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Select UNIQUE Nodal ( so that we can click on ref point of bullet later)
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Slect Velocty:

[image: ]
















Now go  to  the Elements/Nodes tab:
Select EDIT SELECTION:
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Then click on bullet ref point, which highlights:
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The select PLOT:
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