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	Device name
	Interface 
	IP Address 
	Subnet Mask
	Default Gateway

	Server-PT
	NIC
	192.168.1.14
	255.255.255.0
	192.168.1.15

	PC-PT PC1
	NIC
	192.168.1.10
	255.255.255.0
	192.168.1.15

	PC-PT PC2
	NIC
	192.169.1.11
	255.255.255.0
	192.168.1.15

	PC-PT PC3
	NIC
	192.168.1.12
	255.255.255.0
	192.168.1.15

	PC-PT PC4
	NIC
	192.168.1.13
	255.255.255.0
	192.168.1.15

	S960-24TT Switch
	NIC
	N/A
	255.255.255.0
	N/A

	1941 Router
	NIC
	192.168.1.15
	255.255.255.0
	N/A

	2901 Router
	NIC
	192.168.3.1
	255.255.255.0
	N/A

	AccessPoint-PT
	NIC
	N/A
	255.255.255.0
	N/A

	Laptop-PT
	NIC
	192.168.3.2
	255.255.255.0
	192.168.3.1



The table that has been presented above is my devices that I used in my simple network.
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 This screengrab is from when I used the laptop to pining the server, and as you can see the ping was successful.
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 This screengrab shows the successful ping from the server to PC1.
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This is a screenshot of me pinging PC2 from the server.
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This is a screenshot of me pinging PC3 from the server.
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This is a screenshot of a ping from PC4 from the server.
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This is a ping from the server to the laptop.


Logical and physical topology

Logical 
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This is my logical topology.

Physical 

[image: Graphical user interface, diagram

Description automatically generated]
This is my physical topology.
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C:\>ping 192.168.1.12
Pinging 192.168.1.12 with 32 bytes of data:

Reply from 192.168.1.12: bytes=32 time<lms TTL-128
Reply from 192.168.1.12: time<lms
Reply from 192.168.1.12: time<lms
Reply from 192.168.1.12: bytes=32 time<lms TTL-128

Ping statistics for 192.168.1.12
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = Oms, Maximum = Oms, Average = Oms
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C:\>ping 192.168.1.13
Pinging 192.168.1.13 with 32 bytes of data:

Reply from 192.168.1.13:
Reply from 192.168.1.13:
Reply from 192.168.1.13:
Reply from 192.168.1.13:

time<lms
time<lms
time<lms

time<lms

Ping statistics for 192.168.1.13:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = Oms, Maximum = Oms, Average = Oms
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C:\>ping 192.168.3.2
Pinging 192.168.3.2 with 32 bytes of data:

Reply from 192.168.3.2: bytes=32 time=37ms TTL-126
Reply from 192.168.3.2: bytes=32
Reply from 192.168.3.2: bytes=32
Reply from 192.168.3.2: bytes=32

Ping statistics for 192.168.3.2:
Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
Minimum = 32ms, Maximum = 41lms, Average = 37ms
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C:\>ping 192.168.1.11

Pinging 192.168.1.11 with 32 bytes of data:
Reply from 192.168.1.11: time<lms TTL-128
Reply from 192.168.1.11: time<lms TTL-128

Reply from 192.168.1.11: time<lms TTL-128
Reply from 192.168.1.11: bytes=32 time<lms TTL-128

Ping statistics for 192.168.1.11:

Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:

Minimum = Oms, Maximum = Oms, Average = Oms
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