Notes January 10th 2023


Setting up Analogue Rig

Mic on stand – XLR (watch which ends go where) – Mixer – XLR out of mixer (can be 2 for stereo speakers – Amplifier – Speakon (or similar speaker cable) – Speaker

Mixer

Mixers are not complicated, just lots of version of the same thing!
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Channel 1 – Rundown

Input Gain – set how much level the channel on mixer is receiving

EQ – Hi
EQ – Mid
EQ – Low

Auxiliary – send the sound elsewhere using the Aux (often used for monitors)

Pan – set the stereo field (sense of left and right – you have 2 ears!)

Level – master level of that particular channel

Don’t forget that you then have master level controls for the ‘main-outs’ and the ‘auxiliary’.
