UWTSD BLENDED COLOUR DYE LAB NOTES

Total Dye Powder Weight for the Recipe 

….… % Depth of shade ÷ 100 X ………………. dry fabric = grams of …………………………………… dye powder 

Choosing colour blend proportions:








…………………………..  g total dye powder weight for recipe ÷ YOUR TOTAL COLOUR PROPRTIONS = 

…………………..………. g dye powder per proportion

                        
………… parts …………………………………………..…………………………………..……….… x ………………. = ………………. g

………… parts …………………………………………...………………………….……………….… x ………………. = ………………. g

………… parts ………………………………………….…………………….………………………… x ………………. = ………………. g

………… parts ……………………………………………………………………..……………….….. x ………………. = ………………. g 
									           TOTAL =                   
Auxiliaries
                                    0.05 X …………… dry fabric = …………… mls Acetic Acid @ 20% strength

                                     0.2  X ……………. dry fabric = …………... grams of glaubers salt 
Water 
[bookmark: _GoBack]                                      50 X ……………... dry fabric = …………… mls of water
Shading & Making Dye Stocks
When dying paler depths of shade, or blending colour proportions, it can sometimes be difficult to weigh and measure a tiny volume of dye stuffs. 
NOTE: THE SCALES GENERALLY WILL ONLY WEIGH IN INCREMENTS OF 0.1, 0.2, 0.3, 0.4, 0.5… 
To combat this we can create a dye stock solution. Dye stocks are made up of a small amount of dye and water, thus diluting the concentration of colour. 
For example: 
	
0.1 gram of dye 
	
into 10mls of hot water 
	
0.1 ÷ 10 = 0.01 g of colour per ml

	
	
into 100mls of hot water
	
0.1 ÷ 100 = 0.001 g of colour per ml

	
	
into 1000mls of hot water 
	
0.1 ÷ 1000 = 0.0001 g of colour per ml



The above examples of dye stock solutions will mean that for every 1ml of liquid you will have a more dilute concentration of colour. This can be measured using a syringe and added to your overarching recipes. 
