Steven Moore
Networks and Cybersecurity Essentials (ACCA4024) Lab5

Starting VBOX and loading Ubuntu ESS. (Had to enable AMD V in my bios settings!)
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List out the options in your virtual machine menu.
Unclear on which menu you mean.
Find out the IP address of the virtual machine. I used the $ ip a command in the terminal.
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Can you browse the internet? Yes.
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In your own words, how was your experience when setting up Vbox?
It was very easy once I enabled AMD V in my bios settings which allowed Virtual box to launch.
Pros / cons of virtual machines
Pros:
Provides a safe environment for testing.
Can run multiple operating systems.
Cons:
Slower / less efficient.
Can be resource intense on the host machine.
Host machine can infect virtual machines and vice versa.
Part 2 Packet tracer
Setting up DNS records so that users can search using addresses instead of IP addresses.
User sally could not access www.cisco.corp but could access 10.44.1.254. added www.cisco.corp to DNS library so that she can.
Why does email require both SMTP and POP3.
SMTP to send emails and POP3 to receive emails
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cisco@ubuntu:~$ ip a
1: lo: <LOOPBACK,UP,LOWER_UP> mtu 65536 qdisc noqueue state UNKNOWN group defaul
t qlen 1
ink/loopback ©0:00:60:60:00:00 brd 00:00:00:00:60:00
inet 127.0.0.1/8 scope host lo
valid_Lft forever preferred_lft forever
inet6 ::1/128 scope host
valid_Lft forever preferred_lft forever
2: enpos3: <BROADCAST,MULTICAST,UP,LOWER_UP> mtu 1500 qdisc pfifo_fast state UP
group default qlen 1000
Tlink/ether 08:00:27:c0:ef:06 brd Ff:ff:ff:ff:ff:ff
inet 10.6.2.15/24 brd 10.6.2.255 scope global dynamic enpes3
valid_Lft 85957sec preferred_Lft 85957sec
inet6 feBo::a7e5:f452:5d5b:4912/64 scope link
valid_Lft forever preferred_lft forever
cisco@ubunt
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