Questions:
Send a ping request from Branch PC to the Enterprise Web Server. Was it successful? Explain.
Yes - ACL 4 only blocks branch access to HQ LAN 1 not HQ LAN 2

Which ACL statement permitted or denied the ping between these two devices? List the access list name or number, the router on which it was applied, and the specific line that the traffic matched.
ACL - branch_to_hq
Router - Branch
Line - 30

Attempt to ping from PC-1 on the HQ LAN 1 to the Branch Server. Was it successful? Explain.
Not successful - ACL 2 blocks all HQ LAN 1 traffic to the branch server

Which ACL statement permitted or denied the ping between these two devices?
ACL - 111 
Router - HQ 
Line - 10

Open a web browser on the External Server and attempt to bring up a web page stored on the Enterprise Web Server. Is it successful? Explain.
Yes - ACL 1 blocks FTP traffic, not HTTP

Which ACL statement permitted or denied the ping between these two devices?
ACL - 101 
Router - HQ 
Line - 30

From the command line on the Internet User PC, attempt to make an FTP connection to the Branch Server. Is the FTP connection successful?
Yes - ACL 1 only blocks FTP to the enterprise server

Which access list should be modified to prevent users from the Internet to make FTP connections to the Branch Server?
ACL 101

Which statement(s) should be added to the access list to deny this traffic?
access-list 101 deny tcp any host 192.168.2.45 eq FTP

