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Tender Ref. No.: 024TA 

22th April 2022
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Michael Thomas
University of Trinity South Wales
Project Manager

We would like to thank you for the opportunity to tender for your Groundworks package on the ‘Y Fforwm’ Library (Project Ref:16109) at SA1 Marina. We have examined and accept in full the content of the drawing package and in sum, the invitation to tender. We have developed a bill of quantities informed by the drawing pack provided and used our best judgement to fill any potential voids of information at this preliminary stage. It should be noted that any assumptions made, whether full items or quantity only, are subject to re-measure once further information is received or further investigation is available. We confirm that we are fully capable and equipped to achieve the scope of work of Project Ref:16109 to an excellent quality in a timely manner.

It is crucial that we fully explain how we have calculated our tender price index (TPI) increment. It should be noted that the TPI forecast within ‘SPONS 2020 Architect’ and Builders’ Price Book’ have not been exposed to the anomaly which is COVID-19. As depicted in our ‘BCIS Indices’ page, we have included officially published tender price indices from BCIS who reflect the market more accurately. We feel that applying the BSIC TPI increments to our SPONS 2020 rates is a fairer rate representation, which can be seen in our ‘Index Factors’ page. 

Main assumptions:
· We have made the assumption based on the historically industrial use of the site that a relatively large excavation is needed of contaminated land, requiring adequate disposal measures. Further information is needed as to the degree of contamination to inform required level of disposal.
· We have made general assumptions of various materials which have not been explicitly specified. This includes concrete and stone specifications.
· We have made a provisional quantity allowance for steel reinforcement which will likely be required within the ring beam foundation. Further information is required to improve the accuracy of whether this item is needed and if so, to what extent. 
· We have used our best judgment to provide suitable assumptions for drainage materials, depths and lengths which would need to be installed to fully satisfy this typical facility. This includes both internal and external drainage provisions.
· We have assumed a 600mm height external skin of facing brickwork.
· We have assumed an allowance of external works required.

TA Construction Consultancy has become well established as an efficient local contractor. We have achieved a number of notable successful construction projects in recent years, and would like to offer our portfolio. We appreciate the opportunity to offer our tender and look forward to your response

Regards
Toby Adamson 		MD of TA Construction Consultancy
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