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Glossary
· CDM- Construction Design Management 
· LOLER- Lifting Objects and Lifting Equipment 
· PUWER- Provision And Use Of Work Equipment Regulations

Introduction 
This report is going to make you aware of the most important legislation in the construction industry by providing in depth descriptions and where these legislations are most relevant. This report will also make you aware on how health and safety is managed on site and by who it is managed by and also on the project The Crown Place which is a student accommodation block on the out skirts of the SA1 campus in Swansea demonstrate on why the CDM regulations are important to the different parties and what responsibilities the people on site have under these regulations. Health and safety in the modern construction era is a massive factor. As we all know the construction industry is one the most dangerous industries to work in with the second yearly death tally out of all the work industries. For every construction company to succeed on site there must be good health and safety. There are massive consequences handed out for poor health and safety these days from the HSE and these consequences are put in place to stop other accidents happening and to make the industry for people to work in. Even though there are still deths in the construction industry the evolution of the legislations have decreased the number of deaths significantly. 

CDM Regulations 
The CDM regulations are possibly the most important regulations in the industry. The CDM regulations were put into place to ensure communication across the workplace on site and to ensure that risks were managed properly and the correct people are doing the right jobs and the right time. The CDM regulations apply to every single project within the Uk no matter how big or small the project is CDM applies to it and must be followed at every aspect of the project. The CDM regulations were first introduced to the industry in 1994 to provide more health and safety and organisation to the industry. As the industry progressed and became bigger the CDM regulations went through some changes in 2007 and in 2015 which is the latest version of the regulations. Even though the regulations have been changed a couple of times the regulations that were put in place in 1994 still remain under CDM regulations 2015 just more regulations have been added. The main regulations that have been added to the CDM regulations are that the people on site must have the right skills, knowledge and training to be working on the site and with that the people on site must have the correct amount of experience as well with the correct supervision. This regulation was brought into the CDM regulations to reduce the number of people working on site without the correct skills and knowledge to do so as this can cause injuries and could cause the project to not go to plan. The other main regulation that was brought into the CDM regulations is that contractors on site must be provided with the correct information and instructions with the correct supervision carried out by someone who is competent to do so. Without the correct information and instructions for the contractors working on site there is a big possibility for the project not to go to plan and there is a high possibility of someone getting hurt in the process as well. With these regulations brought in it is very important that someone competent is there to supervise the works the contractors are carrying out so that if there is something going wrong or a risk occurs where the possibility of someone getting hurt is high then the supervisor can step in and tell the contractors what the risk is and also what they are doing wrong and what they can do to correct what they are doing (BookMyCourse 2023). 

LOLER Regulations
The LOLER regulation is another important regulation that is very important to the construction industry. LOLER is an abbreviation for Lifting Objects and Lifting Equipment. The LOLER regs apply to lifting objects and also the use of plant such as “cherry pickers” to lift people to complete worker at higher points of a building. The LOLER regulations were put into place so that companies who own, operate or have control over lifting equipment. This means that all companies who plan to carry put any lifting exercises with equipment or without. With most lifting exercises the equipment that is being used belongs to the company therefore the PUWER regulations will also comply only if using the company's equipment. All lifting work must be planned out beforehand so that any risks can be minimised before any work is carried out. The lifting exercises must be supervised by someone who is competent to do so and risk assessments must be done before the work is started. The LOLER regulations are also put into place so to ensure that all the equipment used to carry out any work is fit for purpose to prevent any injuries or the equipment failing whilst carrying out work. To ensure that the equipment is fit for purpose they are marked so that the people using the equipment know that the equipment is safe to use. A record is kept by the site manager to ensure that if any defect occur on the equipment is noted and that the people using are made aware of the equipment with the defects (HSE 2023). 



PUWER Regulations
The PUWER regulations are all to do with the equipment and power tools people use on site and in factories. Where LOLER is to do with lifting and lifting using equipment PUWER loos at whether the equipment is safe to use and how to use the equipment safely. As the construction there are more equipment and tools brought in to make construction easier and faster, but with that comes risks therefore the people using the equipment need to be aware on how to use them and most importantly how to use the equipment safely. The main duty of care for the PUWER regulations fall under the employer as they are expected to provide a safe work place for their employees. The Employer is expected to carry out risk assessments before using any equipment on site to minimise any potential risks that could occur when using the equipment. People that are self employed still need to comply to the PUWER regulations but it is their duty to then carry out the risk assessments so that they're safe whilst doing the work and they must make sure that the equipment is safe to use and compliant to the PUWER regulations. Before using the equipment and to decrease the chance of risk the employers should provide some sort of training so that the people using the equipment know how to use them properly. So that the equipment is compliant with the PUWER regulations they must be checked so that the people using them know that they are safe to use. It depends how often the equipment is checked for example equipment should be checked frequently but equipment that is used more often should be checked more frequently. To minimise the risks whilst using equipment under the PUWER regulations the people should set a time limit as to how long they use power tools for to stop long term injuries, they should be wearing the correct PPE and the equipment should be checked if they are safe to use before hand (HSE 2023). 

How Are The CDM Regulations Relevant to The Crown Place Project? 
As we know the Crown Place project is a big project with a lot of people working on the site at once there for there is a lot of people with responsibilities. On a project of this size there is a lot of pressure on the site manager to do a good job of managing the site correctly and make sure that no one gets hurt. Before anyone goes on site the main duty of the site manager is to ensure that the people are competent to work on the site to ensure this the site manager will check their cscs cards to make sure thry can carry out the work. On a project of this size there will be a lot of people working an different aspects of the building at different times therefore the site manager must ensure that the right people are always working at the right place to make sure that they are carrying their work out properly and correctly. Before any contractors starts on site the site manager must carry out a site induction so that everyone on site is aware of the site and is aware of any potential risks that could occur whilst carrying out their work. The site manager must also carry out a toolbox talk so that everyone on site is up to date with the health and safety regulations. Before any contractors carry out any work on site they must be provided with the correct information therefore on the Crown Place Project the site manager wouls provide the contractors with the relevant drawings and briefs of the work so they can complete their work correctly there must be a supervisor looking over the work so its done safely and correctly. Risk assessments must always be carried out with anyone on site so they are aware of any potential risks that could occur therefore on this project the site manager would go through the works with the person carrying out the works to make them aware of the risks and how they can be avoided (BookMyCourse 2023).

Crown Place Risk Assessments
1, Slips, Trips and Falls whilst carrying materials on site. 
To prevent any slips trips and falls on site the are must be looked over to see if there are any pot holes in the ground so that you cant fall into and check if there are any objects that could cause you to trip up. 
2, Falling off the scaffold. 
As this building is a tall building and working at height is a must. People on the scaffold must ensure that they are clipped on with a harness so that if they do fall off they are protected from falling and hitting the ground. 
3. Using Power Tools. 
People who are using power tools must set time limits for how long they are using them for, a suitable time for using them before having a break is 15 minutes. They must also wear the correct PPE. 

4, Objects falling from height. 
To prevent objects falling from height and potentially hurting someone is to net around the scaffolding and for everyone working on site is wearing the correct PPE at all times. 
5, Lifting heavy materials. 
To reduce the risks whilst carrying and lifting heavy materials is to ensure that they are lifted correctly with your back straight and if equipment is used before using the equipment make sure they are safe and compliant to PUWER regulations. 

Conclusion
This report has given information about the relevant and most important regulations for working on a site. In this report the CDM regulations are also broight into the Crown Place project. 
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