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Addressing Table
	Device
	Interface
	IP Address
	Subnet Mask

	
	VLAN 1
	
	255.255.255.0

	
	VLAN 1
	
	255.255.255.0

	
	NIC
	
	255.255.255.0

	
	NIC
	
	255.255.255.0


Objectives
Configure hostnames and IP addresses on two Cisco Internetwork Operating System (IOS) switches using the command-line interface (CLI).
[bookmark: _GoBack]Use Cisco IOS commands to specify or limit access to the device configurations. 
Use IOS commands to save the running configuration.
Configure two host devices with IP addresses.
Verify connectivity between the two PC end devices.
Scenario
As a recently hired LAN technician, your network manager has asked you to demonstrate your ability to configure a small LAN. Your tasks include configuring initial settings on two switches using the Cisco IOS and configuring IP address parameters on host devices to provide end-to-end connectivity. You are to use two switches and two hosts/PCs on a cabled and powered network.
Requirements
Use a console connection to access each switch.
Name 	 and 	 switches.
Use the 	 password for all lines.
Use the 	 secret password.
Encrypt all clear text passwords.
Include the word warning in the message-of-the-day (MOTD) Banner.
Configure addressing for all devices according to the Addressing Table.
Save your configurations.
Verify connectivity between all devices.
Note: Click Check Results to see your progress. Click Reset Activity to generate a new set of requirements. If you click on this before you complete the activity, all configurations will be lost.
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