	Activity to be Assessed
	Assessment Number

	Floor screeding
	0003

	Persons undertaking or affected by the activity

	

	
	Y
	Employees
	Y
	Contractor
	
	Public
	Y
	Service User
	

	

	
	
	Other …………………………………………………………………………………………….

	Identified Hazards and Associated Risks
	Likelihood
	Severity
	Risk Level

	1
	Slips, trips and falls when walking through construction site
	2
	2
	4

	2
	Musculoskeletal injuries caused by incorrect lifting and handling of screed and associated work equipment
	2
	2
	4

	3
	Use of screed mixer and pump – risk of entrapment with moving part
	2
	3
	6

	4
	Falls over screed pipes
	2
	2
	4

	5
	Burns from exposure to screed
	2
	2
	4

	6
	Eye injury
	2
	3
	6

	Existing Control Measures / Additional Control Measures Required

	1
	Slips, trips and falls – ensure provision of safe access/egress to and from and within the workplace

	2
	Musculoskeletal injuries – where the weight of materials/work equipment cannot be reduced, lifting is necessary by trained persons. Consider using mechanical aids where possible e.g trolley

	3
	Use of screed mixer & pump – equipment to be used by trained persons, and in accordance with the manufacturer’s instruction manual. Where fitted, guards must be maintained in good order and must be in place during the operation of the equipment.

	4
	Falls over screed pipes – pipes to be routed where possible in locations that minimise the risk of trip hazards.

	5
	Burns – refer to COSHH assessment (skin to be covered. Exposure to be minimised where possible/ RPE to be worn when in dust form)

	6
	Eye Injury – eye protection to be worn where is a foreseeable risk to injury, in particular when the screed is in dust form or where there is a risk of splashing

	Reassessment of Activity Hazards 
	Likelihood
	Severity
	Risk Level

	1
	Slips, trips and falls when walking through construction site
	1
	3

	3

	2
	Musculoskeletal injuries caused by incorrect lifting and handling of screed and associated work equipment
	1
	2
	2

	3
	Use of screed mixer and pump – risk of entrapment with moving part
	1
	3
	3

	4
	Falls over screed pipes
	1
	2
	2

	5
	Burns from exposure to screed
	1
	2
	2

	6
	Eye injury
	1
	3
	3
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	Reviews
	Key
	

	Review Date: 
	Likelihood
	Severity
	Severity of Injury
	5
	5Y
	10R
	15
	20
	25

	Reviewed by: 
	1   very     unlikely
2   unlikely
3   likely
4   very likely
5   certainty
	1   nuisance
2   minor
3   medical treatment
4   major
5   fatal
	
	4
	4
	8
	12
	16
	20

	Review Date :
	
	
	
	3
	3
	6G
	9
	12
	15

	Reviewed by:
	
	
	
	2
	2
	4
	6Y
	8
	10Y

	Review Date :
	
	
	
	1
	1
	2
	3
	4
	5G

	Reviewed by:
	
	
	
	0
	1
	2
	3
	4
	5

	Review Date :
	
	
	
	Likelihood of Injury

	Reviewed by:
	
	
	
	Low Risk
	
	Medium Risk
	
	High Risk



