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	Actors:- A list of actors who can engage in the activities described in the use case:-

Manufacturer – delivers packaged system in accordance with legislation and quality guidelines 

Users (tankies) 
· Operates system 
· Reloads system 
· Stores system 

Ordnance board
· Provide specification to manufacturer for desired output of system
· 
Service provider (arm of manufacturing company)  
· Maintains system whilst in service

System (L8) 
·  Functions when required by correct stimulus
· Does not function when incorrect stimulus is provided 
· Does not mass eject (chain fire) 
· Subsystems function on correct time delay
· Subsystems burn for correct duration 
· Subsystem produce area effect of correct size 






	Pre-conditions:- Anything that can be assumed to be true when the use case begins :-
· System is fully operational 
· Users are suitably training and competent 
· System is clear of debris
· System is correctly installed 





	Post-Conditions:- Anything that must be true when the use case is complete.

· System has functioned correctly 
· No injuries have occurred 
· System is not damaged 
· Vehicle system is mounted to is undamaged 
· System is in safe state to be reloaded/removed






	Basic Flow:- The set of steps the actors take to accomplish the goal of the Use Case. A clear description of what the system does in response to each user action.

1. System is loaded and continuity test passed
2. Fire commanded given to system 
3. System fires/ejects sub-system
4. Sub-system functions 
5. System is reloaded








	Alternative Flow:- Captures alternative user/system interactions, such as what happens if data is entered incorrectly.
· Sub system fails to function – no function (misfire/blind),
· functions incorrectly -> not enough smoke production/bad burn
· functions incorrectly -> does not function in free air




	Exception Flow :- The things that can happen to prevent the user from reaching their goal.

· System loaded incorrectly -> does not function 
· System fails to operate -> fouling from elements
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